(export (version D)
  (design
    (source "D:\\Work\\Kicad\\CNC\\BreakoutBoards\\Avec drivers Pololu\\Booster Parallèle\\Transistors.sch")
    (date "4/06/2014 9:05:50")
    (tool "eeschema (2013-07-07 BZR 4022)-stable"))
  (components
    (comp (ref Q1)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8C7A))
    (comp (ref R1)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8C92))
    (comp (ref R6)
      (value 100)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8CA1))
    (comp (ref Q2)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D30))
    (comp (ref R2)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D36))
    (comp (ref R7)
      (value 100)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D3C))
    (comp (ref Q3)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D4C))
    (comp (ref R3)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D52))
    (comp (ref R8)
      (value 100)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D58))
    (comp (ref Q4)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D68))
    (comp (ref R4)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D6E))
    (comp (ref R9)
      (value 100)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538C8D74))
    (comp (ref P2)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC48F))
    (comp (ref P3)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC49E))
    (comp (ref P4)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC593))
    (comp (ref P5)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC5A2))
    (comp (ref P7)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC672))
    (comp (ref P8)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC678))
    (comp (ref P9)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC67E))
    (comp (ref P10)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC684))
    (comp (ref P1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC863))
    (comp (ref R5)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 538EC985))
    (comp (ref P6)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 538ECB36)))
  (libparts
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Device2) (part MOS_P)
      (fields
        (field (name Reference) Q)
        (field (name Value) MOS_P)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num D) (name D) (type passive))
        (pin (num G) (name G) (type input))
        (pin (num S) (name S) (type passive))))
    (libpart (lib Device2) (part R)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical conn)
      (uri C:\Electro\kicad\share\library\conn.lib))
    (library (logical Device2)
      (uri C:\Electro\kicad\share\library\Device2.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref R4) (pin 2))
      (node (ref Q4) (pin G)))
    (net (code 2) (name "")
      (node (ref R9) (pin 1))
      (node (ref Q4) (pin D)))
    (net (code 3) (name VCC)
      (node (ref R5) (pin 1))
      (node (ref Q2) (pin S))
      (node (ref P1) (pin 1))
      (node (ref Q4) (pin S))
      (node (ref Q3) (pin S))
      (node (ref Q1) (pin S)))
    (net (code 4) (name /U2-5)
      (node (ref R5) (pin 2))
      (node (ref P6) (pin 1)))
    (net (code 5) (name /U3-5)
      (node (ref P10) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 6) (name /U3-1)
      (node (ref P9) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 7) (name /U1-4)
      (node (ref R7) (pin 2))
      (node (ref P8) (pin 1)))
    (net (code 8) (name /U1-1)
      (node (ref P7) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 9) (name /17-Enable)
      (node (ref P5) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 10) (name /16-Out2)
      (node (ref R3) (pin 1))
      (node (ref P4) (pin 1)))
    (net (code 11) (name /14-Pwm)
      (node (ref P3) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 12) (name /1-Out1)
      (node (ref R1) (pin 1))
      (node (ref P2) (pin 1)))
    (net (code 13) (name "")
      (node (ref R6) (pin 1))
      (node (ref Q1) (pin D)))
    (net (code 14) (name "")
      (node (ref R2) (pin 2))
      (node (ref Q2) (pin G)))
    (net (code 15) (name "")
      (node (ref R7) (pin 1))
      (node (ref Q2) (pin D)))
    (net (code 16) (name "")
      (node (ref Q1) (pin G))
      (node (ref R1) (pin 2)))
    (net (code 17) (name "")
      (node (ref R3) (pin 2))
      (node (ref Q3) (pin G)))
    (net (code 18) (name "")
      (node (ref Q3) (pin D))
      (node (ref R8) (pin 1)))))