(export (version D)
  (design
    (source "D:/Work/Kicad/CNC/BreakoutBoards/Avec drivers Pololu/Pigi2 - Commande PWM (Alim)/V1/Driver pwm.sch")
    (date "24/06/2014 7:16:35")
    (tool "eeschema (2013-07-07 BZR 4022)-stable"))
  (components
    (comp (ref U1)
      (value UCC27524)
      (libsource (lib Device2) (part UCC27524))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C30FD))
    (comp (ref R3)
      (value 47K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C365F))
    (comp (ref R2)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C366E))
    (comp (ref R4)
      (value 470)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C367D))
    (comp (ref R7)
      (value 10)
      (datasheet /1W)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C368C))
    (comp (ref D2)
      (value 3V3)
      (libsource (lib Device2) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C369B))
    (comp (ref Q2)
      (value BD139)
      (libsource (lib Device2) (part NPN))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C36AA))
    (comp (ref R8)
      (value 10)
      (datasheet /1W)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C3A00))
    (comp (ref C1)
      (value 1µ)
      (libsource (lib Device2) (part CPM))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C420E))
    (comp (ref R10)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 529C42D1))
    (comp (ref R9)
      (value 10)
      (datasheet /1W)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52AE9BEB))
    (comp (ref R6)
      (value 10)
      (datasheet /1W)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52AE9BF1))
    (comp (ref D1)
      (value 4148)
      (libsource (lib Device2) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 539FCF39))
    (comp (ref Q1)
      (value BS250)
      (libsource (lib Device2) (part MOS_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A9097D))
    (comp (ref R5)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A90A74))
    (comp (ref R1)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A90BEB))
    (comp (ref P1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A90FFD))
    (comp (ref P2)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A9100C))
    (comp (ref P3)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A9101B))
    (comp (ref P5)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A9102A))
    (comp (ref P4)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A91039))
    (comp (ref P6)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53A91048)))
  (libparts
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Device2) (part Cpm)
      (fields
        (field (name Reference) C)
        (field (name Value) Cpm)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device2) (part DIODE)
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib Device2) (part MOS_P)
      (fields
        (field (name Reference) Q)
        (field (name Value) MOS_P)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num D) (name D) (type passive))
        (pin (num G) (name G) (type input))
        (pin (num S) (name S) (type passive))))
    (libpart (lib Device2) (part NPN)
      (fields
        (field (name Reference) Q)
        (field (name Value) NPN)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Device2) (part R)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device2) (part UCC27524)
      (fields
        (field (name Reference) U)
        (field (name Value) UCC27524)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ENA) (type input))
        (pin (num 2) (name INA) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name INB) (type input))
        (pin (num 5) (name OUTB) (type output))
        (pin (num 6) (name VDD) (type power_in))
        (pin (num 7) (name OUTA) (type output))
        (pin (num 8) (name ENB) (type input))))
    (libpart (lib Device2) (part ZENER)
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) ZENER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive)))))
  (libraries
    (library (logical conn)
      (uri C:\Electro\kicad\share\library\conn.lib))
    (library (logical Device2)
      (uri C:\Electro\kicad\share\library\Device2.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref Q1) (pin G))
      (node (ref R1) (pin 2)))
    (net (code 2) (name /E_Stop)
      (node (ref D1) (pin 2))
      (node (ref P2) (pin 1)))
    (net (code 3) (name /B_/Enable)
      (node (ref P1) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 4) (name "")
      (node (ref R3) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref Q2) (pin 2)))
    (net (code 5) (name /M_PWM)
      (node (ref P3) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 6) (name "")
      (node (ref D2) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 7) (name "")
      (node (ref Q1) (pin D))
      (node (ref U1) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 8) (name "")
      (node (ref R6) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 9) (name +12V)
      (node (ref U1) (pin 6))
      (node (ref R4) (pin 1))
      (node (ref Q1) (pin S))
      (node (ref C1) (pin 1))
      (node (ref P4) (pin 1)))
    (net (code 10) (name "")
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref R9) (pin 1)))
    (net (code 11) (name /Gate)
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref P5) (pin 1)))
    (net (code 12) (name "")
      (node (ref R4) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref D1) (pin 1)))
    (net (code 13) (name GND)
      (node (ref R10) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref C1) (pin 2))
      (node (ref Q2) (pin 1))
      (node (ref P6) (pin 1)))))