(export (version D)
  (design
    (source "D:/Work/Kicad/CNC/BreakoutBoards/Avec drivers Pololu/TestPololu.sch")
    (date "23/09/2013 15:34:58")
    (tool "eeschema (2013-05-31 BZR 4019)-stable"))
  (components
    (comp (ref Dr1)
      (value StepStick)
      (libsource (lib Device2) (part POLOLUDRIVER))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7E83))
    (comp (ref P2)
      (value MOT)
      (libsource (lib conn) (part CONN_4))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7E89))
    (comp (ref P1)
      (value VMOT)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7E95))
    (comp (ref JP1)
      (value JUMPERM)
      (libsource (lib Device2) (part JUMPERM))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7E9B))
    (comp (ref JP2)
      (value JUMPERM)
      (libsource (lib Device2) (part JUMPERM))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7EA1))
    (comp (ref JP3)
      (value JUMPERM)
      (libsource (lib Device2) (part JUMPERM))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7EA7))
    (comp (ref C5)
      (value 47µ)
      (datasheet /63V)
      (libsource (lib Device2) (part CPM))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7EB9))
    (comp (ref C6)
      (value 100n)
      (libsource (lib Device2) (part CM))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7EBF))
    (comp (ref U2)
      (value LM555)
      (libsource (lib linear) (part LM555))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7ED5))
    (comp (ref C4)
      (value 100nF)
      (libsource (lib Device2) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7EE4))
    (comp (ref C3)
      (value 100nF)
      (libsource (lib Device2) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7EF3))
    (comp (ref R2)
      (value 2K7)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7F02))
    (comp (ref R3)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7F11))
    (comp (ref RV1)
      (value 50K)
      (libsource (lib Device2) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA7F20))
    (comp (ref U1)
      (value LM2576-5V)
      (libsource (lib Device2) (part LM2576))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA82DE))
    (comp (ref D1)
      (value MBR360)
      (libsource (lib Device2) (part DIODESCH))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA82E4))
    (comp (ref C2)
      (value 1000uF)
      (footprint 12,5//5)
      (datasheet 35V)
      (libsource (lib Device2) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA82EA))
    (comp (ref C1)
      (value 100uF)
      (footprint 10//5)
      (datasheet 75V)
      (libsource (lib Device2) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA82F0))
    (comp (ref L1)
      (value 100uH)
      (libsource (lib Device2) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA82F6))
    (comp (ref D2)
      (value 5V)
      (libsource (lib Device2) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA8309))
    (comp (ref R1)
      (value 330)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA830F))
    (comp (ref SW2)
      (value Step)
      (libsource (lib Device2) (part SWITCH_INV))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA891E))
    (comp (ref R4)
      (value 10K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA8C09))
    (comp (ref SW3)
      (value DIR)
      (libsource (lib Device2) (part SWITCH_INV))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA8D21))
    (comp (ref SW4)
      (value ENABLE)
      (libsource (lib Device2) (part SWITCH_INV))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CA8E6C))
    (comp (ref SW1)
      (value Pas)
      (libsource (lib Device2) (part SW_PUSH4))
      (sheetpath (names /) (tstamps /))
      (tstamp 51CC28F6))
    (comp (ref JP4)
      (value JUMPERM)
      (libsource (lib Device2) (part JUMPERM))
      (sheetpath (names /) (tstamps /))
      (tstamp 52404218))
    (comp (ref JP5)
      (value JUMPERM)
      (libsource (lib Device2) (part JUMPERM))
      (sheetpath (names /) (tstamps /))
      (tstamp 52404227))
    (comp (ref JP6)
      (value JUMPERM)
      (libsource (lib Device2) (part JUMPERM))
      (sheetpath (names /) (tstamps /))
      (tstamp 52404236)))
  (libparts
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib Device2) (part C)
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device2) (part Cm)
      (fields
        (field (name Reference) C)
        (field (name Value) Cm))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device2) (part CP)
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device2) (part Cpm)
      (fields
        (field (name Reference) C)
        (field (name Value) Cpm))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device2) (part DIODESCH)
      (fields
        (field (name Reference) D)
        (field (name Value) DIODESCH))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib Device2) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device2) (part JUMPERM)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPERM))
      (pins
        (pin (num 1) (name 1) (type BiDi))
        (pin (num 2) (name 2) (type BiDi))))
    (libpart (lib Device2) (part LED)
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num A) (name A) (type passive))
        (pin (num K) (name K) (type passive))))
    (libpart (lib Device2) (part LM2576)
      (fields
        (field (name Reference) U)
        (field (name Value) LM2576))
      (pins
        (pin (num 1) (name In) (type power_in))
        (pin (num 2) (name Out) (type power_out))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name Feedback) (type input))
        (pin (num 5) (name /On-Off) (type input))))
    (libpart (lib Device2) (part POLOLUDRIVER)
      (fields
        (field (name Reference) Dr)
        (field (name Value) POLOLUDRIVER))
      (pins
        (pin (num 1) (name /Enable) (type input))
        (pin (num 2) (name MS1) (type input))
        (pin (num 3) (name MS2) (type input))
        (pin (num 4) (name MS3) (type input))
        (pin (num 5) (name /RESET) (type input))
        (pin (num 6) (name /SLEEP) (type input))
        (pin (num 7) (name STEP) (type input))
        (pin (num 8) (name DIR) (type input))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name VDD) (type power_in))
        (pin (num 11) (name 1B) (type power_out))
        (pin (num 12) (name 1A) (type power_out))
        (pin (num 13) (name 2A) (type power_out))
        (pin (num 14) (name 2B) (type power_out))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name VMOT) (type power_in))))
    (libpart (lib Device2) (part POT)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device2) (part R)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device2) (part SW_PUSH4)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH4))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Device2) (part SWITCH_INV)
      (fields
        (field (name Reference) SW)
        (field (name Value) SWITCH_INV))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib linear) (part LM555)
      (docs ns/lm555.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) LM555))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name TR) (type input))
        (pin (num 3) (name Q) (type output))
        (pin (num 4) (name R) (type input))
        (pin (num 5) (name CV) (type input))
        (pin (num 6) (name THR) (type input))
        (pin (num 7) (name DIS) (type input))
        (pin (num 8) (name VCC) (type power_in)))))
  (libraries
    (library (logical Device2)
      (uri C:\Electro\kicad\share\library\Device2.lib))
    (library (logical conn)
      (uri C:\Electro\kicad\share\library\conn.lib))
    (library (logical linear)
      (uri C:\Electro\kicad\share\library\linear.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref RV1) (pin 3)))
    (net (code 2) (name "")
      (node (ref Dr1) (pin 6))
      (node (ref Dr1) (pin 5)))
    (net (code 3) (name "")
      (node (ref U2) (pin 7))
      (node (ref R3) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 4) (name /Out5)
      (node (ref U1) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref L1) (pin 1)))
    (net (code 5) (name "")
      (node (ref D2) (pin A))
      (node (ref R1) (pin 2)))
    (net (code 6) (name "")
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 7) (name GND)
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 3))
      (node (ref D1) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref SW4) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref SW3) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref Dr1) (pin 9))
      (node (ref C6) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref Dr1) (pin 15))
      (node (ref C5) (pin 2))
      (node (ref D2) (pin K)))
    (net (code 8) (name "")
      (node (ref U2) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref RV1) (pin 2))
      (node (ref U2) (pin 6)))
    (net (code 9) (name "")
      (node (ref RV1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 10) (name STEPb)
      (node (ref Dr1) (pin 7))
      (node (ref JP5) (pin 2)))
    (net (code 11) (name VCC)
      (node (ref C6) (pin 1))
      (node (ref JP3) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 4))
      (node (ref R2) (pin 1))
      (node (ref Dr1) (pin 10))
      (node (ref JP1) (pin 1))
      (node (ref JP2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref SW1) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref SW4) (pin 3))
      (node (ref R1) (pin 1))
      (node (ref SW3) (pin 3))
      (node (ref L1) (pin 2)))
    (net (code 12) (name ENABLEa)
      (node (ref SW4) (pin 2))
      (node (ref JP4) (pin 1)))
    (net (code 13) (name ENABLEb)
      (node (ref Dr1) (pin 1))
      (node (ref JP4) (pin 2)))
    (net (code 14) (name STEPa)
      (node (ref R4) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref JP5) (pin 1)))
    (net (code 15) (name DIRa)
      (node (ref JP6) (pin 1))
      (node (ref SW3) (pin 2)))
    (net (code 16) (name DIRb)
      (node (ref JP6) (pin 2))
      (node (ref Dr1) (pin 8)))
    (net (code 17) (name /Auto)
      (node (ref U2) (pin 3))
      (node (ref SW2) (pin 3)))
    (net (code 18) (name /Man)
      (node (ref SW1) (pin 4))
      (node (ref SW1) (pin 3))
      (node (ref SW2) (pin 1)))
    (net (code 19) (name /s2)
      (node (ref Dr1) (pin 3))
      (node (ref JP2) (pin 2)))
    (net (code 20) (name /s1)
      (node (ref Dr1) (pin 2))
      (node (ref JP1) (pin 2)))
    (net (code 21) (name /1b)
      (node (ref P2) (pin 4))
      (node (ref Dr1) (pin 11)))
    (net (code 22) (name /1a)
      (node (ref P2) (pin 3))
      (node (ref Dr1) (pin 12)))
    (net (code 23) (name /2a)
      (node (ref P2) (pin 2))
      (node (ref Dr1) (pin 13)))
    (net (code 24) (name /2b)
      (node (ref P2) (pin 1))
      (node (ref Dr1) (pin 14)))
    (net (code 25) (name VAA)
      (node (ref C1) (pin 1))
      (node (ref Dr1) (pin 16))
      (node (ref U1) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref C5) (pin 1)))
    (net (code 26) (name /s3)
      (node (ref Dr1) (pin 4))
      (node (ref JP3) (pin 2)))))