Cmp-Mod V01 Created by CvPcb (2012-01-19 BZR 3256)-stable date = 1/10/2012 10:55:13

BeginCmp
TimeStamp = /5066ADAD;
Reference = C1;
ValeurCmp = 100n;
IdModule  = C050-024X044;
EndCmp

BeginCmp
TimeStamp = /5066ADB1;
Reference = C2;
ValeurCmp = 100n;
IdModule  = C050-024X044;
EndCmp

BeginCmp
TimeStamp = /506953E1;
Reference = C3;
ValeurCmp = 470µ;
IdModule  = E3,5-10;
EndCmp

BeginCmp
TimeStamp = /506953F2;
Reference = C4;
ValeurCmp = 100n;
IdModule  = C050-024X044;
EndCmp

BeginCmp
TimeStamp = /506953EF;
Reference = C5;
ValeurCmp = 100n;
IdModule  = C050-024X044;
EndCmp

BeginCmp
TimeStamp = /506953E5;
Reference = C6;
ValeurCmp = 220µ;
IdModule  = E3,5-8;
EndCmp

BeginCmp
TimeStamp = /505FEC53;
Reference = P1;
ValeurCmp = M25;
IdModule  = DB25MC;
EndCmp

BeginCmp
TimeStamp = /506953B5;
Reference = P2;
ValeurCmp = CONN_2;
IdModule  = MSTBV2;
EndCmp

BeginCmp
TimeStamp = /50606C55;
Reference = P3;
ValeurCmp = Digital1;
IdModule  = FE08;
EndCmp

BeginCmp
TimeStamp = /50606C59;
Reference = P4;
ValeurCmp = Digital2;
IdModule  = FE08;
EndCmp

BeginCmp
TimeStamp = /50606C6C;
Reference = P5;
ValeurCmp = Alim;
IdModule  = FE06;
EndCmp

BeginCmp
TimeStamp = /50606C72;
Reference = P6;
ValeurCmp = Analog;
IdModule  = FE06;
EndCmp

BeginCmp
TimeStamp = /505FEC90;
Reference = R1;
ValeurCmp = 2K2;
IdModule  = R0207-0100;
EndCmp

BeginCmp
TimeStamp = /505FEC8F;
Reference = R2;
ValeurCmp = 2K2;
IdModule  = R0207-0100;
EndCmp

BeginCmp
TimeStamp = /505FEC8E;
Reference = R3;
ValeurCmp = 2K2;
IdModule  = R0207-0100;
EndCmp

BeginCmp
TimeStamp = /505FEC8D;
Reference = R4;
ValeurCmp = 2K2;
IdModule  = R0207-0100;
EndCmp

BeginCmp
TimeStamp = /505FEC8C;
Reference = R5;
ValeurCmp = 2K2;
IdModule  = R0207-0100;
EndCmp

BeginCmp
TimeStamp = /505FECB7;
Reference = R6;
ValeurCmp = 330;
IdModule  = R0207-0400;
EndCmp

BeginCmp
TimeStamp = /505FECB8;
Reference = R7;
ValeurCmp = 330;
IdModule  = R0207-0400;
EndCmp

BeginCmp
TimeStamp = /505FECB9;
Reference = R8;
ValeurCmp = 330;
IdModule  = R0207-0400;
EndCmp

BeginCmp
TimeStamp = /505FECBA;
Reference = R9;
ValeurCmp = 330;
IdModule  = R0207-0400;
EndCmp

BeginCmp
TimeStamp = /505FECBB;
Reference = R10;
ValeurCmp = 330;
IdModule  = R0207-0400;
EndCmp

BeginCmp
TimeStamp = /505FEC89;
Reference = RP1;
ValeurCmp = 4X330;
IdModule  = DIL08;
EndCmp

BeginCmp
TimeStamp = /505FEC8A;
Reference = RP2;
ValeurCmp = 4X330;
IdModule  = DIL08;
EndCmp

BeginCmp
TimeStamp = /505FEC8B;
Reference = RP3;
ValeurCmp = 4X330;
IdModule  = DIL08;
EndCmp

BeginCmp
TimeStamp = /505FEC84;
Reference = U1;
ValeurCmp = OPTO4;
IdModule  = DIL16;
EndCmp

BeginCmp
TimeStamp = /505FEC88;
Reference = U2;
ValeurCmp = OPTO1;
IdModule  = DIL06;
EndCmp

BeginCmp
TimeStamp = /505FEC85;
Reference = U3;
ValeurCmp = OPTO4;
IdModule  = DIL16;
EndCmp

BeginCmp
TimeStamp = /505FEC86;
Reference = U4;
ValeurCmp = OPTO4;
IdModule  = DIL16;
EndCmp

BeginCmp
TimeStamp = /505FEC87;
Reference = U5;
ValeurCmp = OPTO4;
IdModule  = DIL16;
EndCmp

BeginCmp
TimeStamp = /505FECB6;
Reference = U6;
ValeurCmp = ULN2003;
IdModule  = DIL16;
EndCmp

BeginCmp
TimeStamp = /50615A5B;
Reference = U7;
ValeurCmp = 74LS540;
IdModule  = DIL20;
EndCmp

BeginCmp
TimeStamp = /50615A8A;
Reference = U8;
ValeurCmp = 74LS540;
IdModule  = DIL20;
EndCmp

BeginCmp
TimeStamp = /50695418;
Reference = U9;
ValeurCmp = 7805;
IdModule  = TO220;
EndCmp

BeginCmp
TimeStamp = /505FEC56;
Reference = USB-B1;
ValeurCmp = ALIM_5V;
IdModule  = USB-B;
EndCmp

EndListe
