(export (version D)
  (design
    (source "D:\\Work\\Kicad\\CNC\\BreakoutBoards\\Avec drivers Pololu\\Pigi3 - Entrées\\V1\\Entrées.sch")
    (date "9/07/2014 9:07:39")
    (tool "eeschema (2013-07-07 BZR 4022)-stable"))
  (components
    (comp (ref C1)
      (value 270p)
      (libsource (lib Device2) (part CAP3F))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC369B))
    (comp (ref D3)
      (value In3)
      (libsource (lib Device2) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC36DB))
    (comp (ref D4)
      (value In4)
      (libsource (lib Device2) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC36E1))
    (comp (ref D2)
      (value In2)
      (libsource (lib Device2) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC36F3))
    (comp (ref D1)
      (value In1)
      (libsource (lib Device2) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC36F9))
    (comp (ref Q1)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3A68))
    (comp (ref C2)
      (value 270p)
      (libsource (lib Device2) (part CAP3F))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3B4B))
    (comp (ref Q2)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3B51))
    (comp (ref C3)
      (value 270p)
      (libsource (lib Device2) (part CAP3F))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3B7D))
    (comp (ref Q3)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3B83))
    (comp (ref C4)
      (value 270p)
      (libsource (lib Device2) (part CAP3F))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3C07))
    (comp (ref Q4)
      (value BS250)
      (libsource (lib Device2) (part MOSFET_P))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC3C0D))
    (comp (ref R1)
      (value 4K7)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC510E))
    (comp (ref R3)
      (value 4K7)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AC52EC))
    (comp (ref P1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD520D))
    (comp (ref P2)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD66F0))
    (comp (ref P3)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD66F6))
    (comp (ref P4)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD66FC))
    (comp (ref D8)
      (value 5V1)
      (libsource (lib Device2) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD6F49))
    (comp (ref R9)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD738D))
    (comp (ref D7)
      (value 5V1)
      (libsource (lib Device2) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD739D))
    (comp (ref D6)
      (value 5V1)
      (libsource (lib Device2) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD73A3))
    (comp (ref D5)
      (value 5V1)
      (libsource (lib Device2) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD73A9))
    (comp (ref R2)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD87A1))
    (comp (ref P9)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD87A7))
    (comp (ref P10)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD87AD))
    (comp (ref P11)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD87B3))
    (comp (ref P12)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD87B9))
    (comp (ref R10)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD883C))
    (comp (ref R11)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD8842))
    (comp (ref R12)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD8848))
    (comp (ref R8)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD88AD))
    (comp (ref R6)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD88B3))
    (comp (ref R4)
      (value 1K)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53AD88B9))
    (comp (ref P13)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE4B0))
    (comp (ref P14)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE4BF))
    (comp (ref P15)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE4C5))
    (comp (ref P16)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE4CB))
    (comp (ref P5)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE6B7))
    (comp (ref P6)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE6BD))
    (comp (ref P7)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE6C3))
    (comp (ref P8)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCE6C9))
    (comp (ref R7)
      (value 4K7)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCF8A5))
    (comp (ref R5)
      (value 4K7)
      (libsource (lib Device2) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BCF8AB)))
  (libparts
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Device2) (part CAP3F)
      (fields
        (field (name Reference) C)
        (field (name Value) CAP3F)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type BiDi))
        (pin (num 2) (name C) (type BiDi))
        (pin (num 3) (name B) (type BiDi))))
    (libpart (lib Device2) (part LED)
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num A) (name A) (type passive))
        (pin (num K) (name K) (type passive))))
    (libpart (lib Device2) (part MOS_P)
      (fields
        (field (name Reference) Q)
        (field (name Value) MOS_P)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num D) (name D) (type passive))
        (pin (num G) (name G) (type input))
        (pin (num S) (name S) (type passive))))
    (libpart (lib Device2) (part R)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device2) (part ZENER)
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) ZENER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive)))))
  (libraries
    (library (logical conn)
      (uri C:\Electro\kicad\share\library\conn.lib))
    (library (logical Device2)
      (uri C:\Electro\kicad\share\library\Device2.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref R2) (pin 1))
      (node (ref D1) (pin K)))
    (net (code 2) (name "")
      (node (ref D4) (pin K))
      (node (ref R8) (pin 1)))
    (net (code 3) (name GND)
      (node (ref C4) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref D5) (pin 1))
      (node (ref P13) (pin 1))
      (node (ref P14) (pin 1))
      (node (ref P15) (pin 1))
      (node (ref P16) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref D6) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref D8) (pin 1))
      (node (ref C2) (pin 2)))
    (net (code 4) (name "")
      (node (ref D2) (pin K))
      (node (ref R4) (pin 1)))
    (net (code 5) (name "")
      (node (ref C4) (pin 3))
      (node (ref P4) (pin 1)))
    (net (code 6) (name "")
      (node (ref D8) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref P12) (pin 1)))
    (net (code 7) (name "")
      (node (ref D7) (pin 2))
      (node (ref R11) (pin 1))
      (node (ref P11) (pin 1)))
    (net (code 8) (name "")
      (node (ref P10) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref D6) (pin 2)))
    (net (code 9) (name "")
      (node (ref P9) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 10) (name "")
      (node (ref C4) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref Q4) (pin G)))
    (net (code 11) (name "")
      (node (ref C3) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref Q3) (pin G)))
    (net (code 12) (name "")
      (node (ref P3) (pin 1))
      (node (ref C3) (pin 3)))
    (net (code 13) (name +12V)
      (node (ref R3) (pin 2))
      (node (ref Q1) (pin S))
      (node (ref R1) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref P5) (pin 1))
      (node (ref P6) (pin 1))
      (node (ref P7) (pin 1))
      (node (ref P8) (pin 1))
      (node (ref Q2) (pin S))
      (node (ref Q3) (pin S))
      (node (ref Q4) (pin S)))
    (net (code 14) (name "")
      (node (ref R12) (pin 2))
      (node (ref Q4) (pin D))
      (node (ref D4) (pin A)))
    (net (code 15) (name "")
      (node (ref Q3) (pin D))
      (node (ref D3) (pin A))
      (node (ref R11) (pin 2)))
    (net (code 16) (name "")
      (node (ref R6) (pin 1))
      (node (ref D3) (pin K)))
    (net (code 17) (name "")
      (node (ref D2) (pin A))
      (node (ref R10) (pin 2))
      (node (ref Q2) (pin D)))
    (net (code 18) (name "")
      (node (ref Q1) (pin D))
      (node (ref D1) (pin A))
      (node (ref R9) (pin 2)))
    (net (code 19) (name "")
      (node (ref R3) (pin 1))
      (node (ref Q2) (pin G))
      (node (ref C2) (pin 1)))
    (net (code 20) (name "")
      (node (ref P1) (pin 1))
      (node (ref C1) (pin 3)))
    (net (code 21) (name "")
      (node (ref C2) (pin 3))
      (node (ref P2) (pin 1)))
    (net (code 22) (name "")
      (node (ref C1) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref Q1) (pin G)))))